DICOM PS3.4 2016d - Service Class Specifications

P.2.2.4 Status Codes
Prev | P.2.2 Operation | Next

#### P.2.2.4 Status Codes

The Service Class specific status values defined for the N-ACTION Service are specified in Table P.2-3. See PS3.7 for additional general response status codes.

Table P.2-3. Response Status

Service Status | Response Status Code | Further Meaning
--- | --- | ---
Success | 0000 |
Warning | B101 | Specified Synchronization Frame of Reference UID does not match SCP Synchronization Frame of Reference
Warning | B102 | Study Instance UID coercion; Event logged under a different Study Instance UID
Warning | B104 | IDs inconsistent in matching a current study; Event logged
Failure | C101 | Procedural Logging not available for specified Study Instance UID
Failure | C102 | Event Information does not match Template
Failure | C103 | Cannot match event to a current study
Failure | C104 | IDs inconsistent in matching a current study; Event not logged

Prev | Up | Next
P.2.2.3 Service Class Provider Behavior | Home | P.2.2.5 Action Reply

DICOM PS3.4 2016d - Service Class Specifications