DICOM PS3.16 2016d - Content Mapping Resource

TID 3208 Frame-to-Frame Results
Prev | Quantitative Ventricular Analysis Report SR IOD Templates | Next

### TID 3208 Frame-to-Frame Results

The Frame-to-Frame Result Template consists of a CONTAINER providing measurements derived from the angiographic images on frame-by-frame basis.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3208. Frame-To-Frame Result

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122499, DCM, "Frame to Frame Analysis")
3 | > | CONTAINS | IMAGE | EV (121112, DCM, "Source of Measurement") | 1-2 | M | VM = 1: Single plane analysis, VM = 2: Biplane analysis |
4 | > | CONTAINS | CODE | EV (122429, DCM, "Volume Method") | 1 | M |  | DCID 3453 “Cardiac Volume Methods”
5 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | M |  | $Measurement = DCID 3471 “Estimated Volumes” $TargetSite = DCID 3462 “Chamber Identification” $Unit = DT (ml, UCUM, "ml")
6 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (122445, DCM, "Wall Thickness") $Unit = DT (mm, UCUM, "mm")
7 | > | CONTAINS | IMAGE | No purpose of reference | 1-n | U |  |

Content Item Descriptions

Row 3 | Identifies each frame analyzed, using the multi-valued Referenced Frame Number (0008,1160) attribute of the IMAGE Content Item.
Row 5, 6 | Includes one measurement for each frame referenced in Row 3.
Row 7 | Secondary Capture image with ventricular contours

Prev | Up | Next
TID 3207 AA Main Results | Home | TID 3209 Centerline Wall Motion

DICOM PS3.16 2016d - Content Mapping Resource