DICOM PS3.7 2016d - Message Exchange

C.2 Pending Status Class
Prev | C Status Type Encoding (Normative) | Next

## C.2 Pending Status Class

Statuses in this Status Class convey that the operation/notification is continuing and additional Statuses are expected.

### C.2.1 Pending

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.

Prev | Up | Next
C Status Type Encoding (Normative) | Home | C.3 Cancel Status Class

DICOM PS3.7 2016d - Message Exchange