DICOM PS3.3 2016d - Information Object Definitions

F.5.43 Surface Scan Mesh Directory Record Definition
Prev | F.5 Definition of Specific Directory Records | Next

### F.5.43 Surface Scan Mesh Directory Record Definition

The Directory Record is based on the specification of Section F.3. It is identified by a Directory Record Type of Value "SURFACE SCAN". Table F.5-43 lists the set of keys with their associated Types for such a Directory Record Type. The description of these keys may be found in the Modules related to the Surface IE of the Surface Scan Mesh and Surface Scan Point Cloud IODs. This Directory Record shall be used to reference a Surface Scan Mesh SOP Instance. This type of Directory Record may reference a Lower-Level Directory Entity that includes one or more Directory Records as defined in Table F.4-1.

Table F.5-43. Surface Scan Keys

Key | Tag | Type | Attribute Description
--- | --- | --- | ---
Specific Character Set | (0008,0005) | 1C | Required if an extended or replacement character set is used in one of the keys.
Content Date | (0008,0023) | 1 | The date the content creation started.
Content Time | (0008,0033) | 1 | The time the content creation started.
Any other Attribute of the Surface IE Modules | 3 |

### Note

Because (0004,1511) Referenced SOP Instance UID in File may be used as a "pseudo" Directory Record Key (see Table F.3-3), it is not duplicated in this list of keys.

Prev | Up | Next
F.5.42 Surface Directory Record Definition | Home | F.5.44 Tractography Results Directory Record Definition

DICOM PS3.3 2016d - Information Object Definitions