DICOM PS3.4 2016d - Service Class Specifications

N.2.5.2 Edge Enhancement
Prev | N.2.5 Angiography Grayscale Transformations | Next

#### N.2.5.2 Edge Enhancement

The Edge Enhancement transformation consists of filter operations to enhance the display of the pixel data as specified by the Attribute Display Filter Percentage of the XA/XRF Presentation State Presentation Module.

Prev | Up | Next
N.2.5 Angiography Grayscale Transformations | Home | N.3 Behavior of an SCP

DICOM PS3.4 2016d - Service Class Specifications