DICOM PS3.3 2016d - Information Object Definitions

A.66.3 Intravascular OCT Image IOD Modules
Prev | A.66 Intravascular OCT IOD | Next

### A.66.3 Intravascular OCT Image IOD Modules

Table A.66.3-1 specifies the Modules of the Intravascular Optical Coherence Tomography Image IOD.

Table A.66.3-1. Intravascular OCT Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Intravascular OCT Series | C.8.27.1 | M
Frame of Reference | Frame of Reference | C.7.4.1 | M
Synchronization | C.7.4.2 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Image Pixel | C.7.6.3 | M
Supplemental Palette Color Lookup Table | C.7.6.19 | C - Required if Pixel Presentation (0008,9205) in the Intravascular OCT Image Module equals COLOR.
Enhanced Contrast/Bolus | C.7.6.4 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | M
Device | C.7.6.12 | U
Acquisition Context | C.7.6.14 | M
Cardiac Synchronization | C.7.6.18.1 | C - Required if cardiac synchronization was used
Intravascular OCT Image | C.8.27.2 | M
Intravascular OCT Acquisition Parameters | C.8.27.3 | M
Intravascular OCT Processing Parameters | C.8.27.4 | C - Required if Presentation Intent Type (0008,0068) is FOR PROCESSING.
Intravascular Image Acquisition Parameters | C.8.27.5 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | M
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

#### A.66.3.1 Intravascular OCT Image IOD Content Constraints

The following constraints on Image attributes take precedence over the descriptions given in the Module Attribute Tables.

##### A.66.3.1.1 Contrast/Bolus Agent Sequence

For Contrast/Bolus Agent Sequence (0018,0012), the Defined Context Group is 3850.

##### A.66.3.1.2 Prohibited Modules

The Overlay Plane Module and VOI LUT Module shall not be used in a Standard Extended SOP Class of the Intravascular Optical Coherence Tomography Image.

### Note

In order to annotate images, whether during acquisition or subsequently, SOP Instances of the Grayscale Softcopy Presentation State Storage or the Structured Report Storage SOP Classes that reference the image SOP Instance may be used.

Pseudo-color presentation information may be applied through the use of separate Pseudo-color Softcopy Presentation State SOP instances.

No standard mechanism is provided for inclusion of annotations within the image SOP Instance itself and implementers are discouraged from using private extensions to circumvent this restriction.

Prev | Up | Next
A.66.2 Intravascular OCT Image IOD Entity-Relationship Model | Home | A.66.4 Intravascular OCT Image Functional Group Macros

DICOM PS3.3 2016d - Information Object Definitions