DICOM PS3.3 2016d - Information Object Definitions

A.56.3 Enhanced PET Image IOD Module Table
Prev | A.56 Enhanced PET Image IOD | Next

### A.56.3 Enhanced PET Image IOD Module Table

Table A.56-1 specifies the Modules of the Enhanced PET Image IOD.

Table A.56-1. Enhanced PET Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Enhanced PET Series | C.8.22.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | M
Synchronization | C.7.4.2 | C - Required if time synchronization was applied.
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Image Pixel | C.7.6.3 | M
Intervention | C.7.6.13 | U
Acquisition Context | C.7.6.14 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | M
Cardiac Synchronization | C.7.6.18.1 | C - Required if cardiac synchronization was applied.
Respiratory Synchronization | C.7.6.18.2 | C - Required if respiratory synchronization was applied.
Specimen | C.7.6.22 | U
Enhanced PET Isotope | C.8.22.4 | M
Enhanced PET Acquisition | C.8.22.2 | M
Enhanced PET Image | C.8.22.3 | M
Enhanced PET Corrections | C.8.22.6 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

#### A.56.3.1 Enhanced PET Image IOD Content Constraints

Modality (0008,0060) shall have the value PT.

The General Image Module, Overlay Plane Module, VOI LUT Module, Supplemental Palette Color Lookup Table Module, and the Softcopy Presentation LUT Module shall not be used in a Standard Extended SOP Class of the Enhanced PET Image.

### Note

1. In order to annotate images, whether during acquisition or subsequently, SOP Instances of the Grayscale Softcopy Presentation State Storage, Color Softcopy Presentation State Storage, or the Structured Report Storage SOP Classes that reference the image SOP Instance, may be used.

2. No standard mechanism is provided for inclusion of annotations within the image SOP Instance itself, and implementers are discouraged from using private extensions to circumvent this restriction.

3. The Blending Softcopy Presentation State and Spatial Registration SOP Classes can be used to relate this SOP Instance to related image, registration, or fiducial SOP Instances.

4. If contrast was administered during a CT acquisition used for attenuation correction, this information can be obtained from the CT SOP Instances and is not encoded in the PET SOP Instances.

Prev | Up | Next
A.56.2 Enhanced PET Image IOD Entity-Relationship Model | Home | A.56.4 Enhanced PET Image Functional Group Macros

DICOM PS3.3 2016d - Information Object Definitions