DICOM PS3.15 2016d - Security and System Management Profiles

A.5.2.4 Multi-homed Nodes
Prev | A.5.2 General Message Format Conventions | Next

#### A.5.2.4 Multi-homed Nodes

The NetworkAccessPointTypeCode and NetworkAccessPointID can be ambiguous for systems that have multiple physical network connections. For these multi-homed nodes a single DNS name or IP address shall be selected and used when reporting audit events. DICOM does not require the use of a specific method for selecting the network connection to be used for identification, but it must be the same for all of the audit messages generated for events on that node.

Prev | Up | Next
A.5.2.3 Username | Home | A.5.2.5 EventDateTime

DICOM PS3.15 2016d - Security and System Management Profiles