DICOM PS3.4 2016d - Service Class Specifications

CC.2.2.4 Status Codes
Prev | CC.2.2 Request UPS Cancel (N-ACTION) | Next

#### CC.2.2.4 Status Codes

The status values that are specific for this DIMSE operation are defined in Table CC.2.2-2.

Table CC.2.2-2. Status Values

Status | Meaning | Code
--- | --- | ---
Success | The cancel request is acknowledged | 0000
Warning | The UPS is already in the requested state of CANCELED | B304
Failure | Refused: The UPS is already COMPLETED | C311
Refused: Performer chooses not to cancel | C313
Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307
Refused: The performer cannot be contacted | C312

Prev | Up | Next
CC.2.2.3 Service Class Provider Behavior | Home | CC.2.3 Subscribe/Unsubscribe to Receive UPS Event Reports (N-ACTION)

DICOM PS3.4 2016d - Service Class Specifications