DICOM PS3.4 2016e - Service Class Specifications

H.4.11.2 DIMSE Service Group
Prev | H.4.11 Printer Configuration Retrieval SOP Class | Next

#### H.4.11.2 DIMSE Service Group

The DIMSE Services that are applicable to the IOD are shown in Table H.4.11.2-1.

Table H.4.11.2-1. IOD DIMSE Services

DIMSE Service Element | Usage SCU/SCP
--- | ---
N-GET | M/M

The meaning of the Usage SCU/SCP is described in Section H.2.4.

This Section describes the behavior of the DIMSE Service that are specific for this IOD. The general behavior of the DIMSE Services is specified in PS3.7.

##### H.4.11.2.2 N-GET

The N-GET is used to retrieve an instance of the Printer Configuration Retrieval SOP Class.

###### H.4.11.2.2.1 Attributes

The Attributes that are retrieved are shown in Table H.4-26.

Table H.4-26. N-GET Attributes

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Printer Configuration Sequence | (2000,001E) | U/M
>SOP Classes Supported | (0008,115A) | -/M
>Maximum Memory Allocation | (2000,0061) | -/M
>Memory Bit Depth | (2000,00A0) | -/M
>Printing Bit Depth | (2000,00A1) | -/M
>Media Installed Sequence | (2000,00A2) | -/M
>>Item Number | (0020,0019) | -/M
>>Medium Type | (2000,0030) | -/M
>>Film Size ID | (2010,0050) | -/M
>>Min Density | (2010,0120) | -/MC Required if Sequence is Present and Min Density is known
>>Max Density | (2010,0130) | -/M
>Other Media Available Sequence | (2000,00A4) | -/M
>>Medium Type | (2000,0030) | -/M
>>Film Size ID | (2010,0050) | -/M
>>Min Density | (2010,0120) | -/MC Required if Sequence is Present and Min Density is known
>>Max Density | (2010,0130) | -/M
>Supported Image Display Formats Sequence | (2000,00A8) | -/M
>>Rows | (0028,0010) | -/MC Required if all Image Boxes in the Display Format have the same number of rows and columns
>>Columns | (0028,0011) | -/MC Required if all Image Boxes in the Display Format have the same number of rows and columns
>>Image Display Format | (2010,0010) | -/M
>>Film Orientation | (2010,0040) | -/M
>>Film Size ID | (2010,0050) | -/M
>>Printer Resolution ID | (2010,0052) | -/M
>>Printer Pixel Spacing | (2010,0376) | -/M
>>Requested Image Size Flag | (2020,00A0) | -/M
>Default Printer Resolution ID | (2010,0054) | -/M
>Default Magnification Type | (2010,00A6) | -/M
>Other Magnification Types Available | (2010,00A7) | -/M
>Default Smoothing Type | (2010,00A8) | -/M
>Other Smoothing Types Available | (2010,00A9) | -/M
>Configuration Information Description | (2010,0152) | -/M
>Maximum Collated Films | (2010,0154) | -/M
>Decimate/Crop Result | (2020,00A2) | -/M
>Manufacturer | (0008,0070) | -/M
>Manufacturer Model Name | (0008,1090) | -/M
>Printer Name | (2110,0030) | -/M

The meaning of the Usage SCU/SCP is described in Section H.2.4.

###### H.4.11.2.2.2 Behavior

The SCU uses the N-GET to request the SCP to get a Printer Configuration Retrieval SOP Instance. The SCU shall specify in the N-GET request primitive the UID of the SOP Instance to be retrieved.

The SCP shall return the values for the specified Attributes of the specified SOP Instance.

The SCP shall return the status code of the requested SOP Instance retrieval.

A Failure status code shall indicate that the SCP has not retrieved the SOP Instance.

Prev | Up | Next
H.4.11 Printer Configuration Retrieval SOP Class | Home | H.4.11.3 SOP Class Definition and UID

DICOM PS3.4 2016e - Service Class Specifications