DICOM PS3.4 2016e - Service Class Specifications

DD.3.2.2.3 Status
Prev | DD.3.2.2 N-GET | Next

##### DD.3.2.2.3 Status

The status values that are specific for these SOP Classes are defined as follows:

Table DD.3.2.2.3-1. RT Conventional Machine and RT Ion Machine Verification SOP Class N-GET Status Values

Status | Meaning | Code
--- | --- | ---
Success | Treatment Verification Status of the applicable Machine Verification instance successfully returned. | 0000
Failure | No such object instance - applicable Machine Verification instance not found | C112

Prev | Up | Next
DD.3.2.2.2 Attributes | Home | DD.3.2.2.4 Behavior

DICOM PS3.4 2016e - Service Class Specifications