DICOM PS3.17 2016e - Explanatory Information

TTT.2.2.4 Example
Prev | TTT.2.2 Case #2: Reconstruction From A Sub-set of Projection Frames | Next

#### TTT.2.2.4 Example

This specific example is the reconstruction of a volume by a back-projection from every 5th frame of a rotational acquisition and encoded as an Enhanced XA Image.

### Note

The example would be very similar if the rotational acquisition was encoded as an XA Image.

Figure TTT.2.2-2. Attributes of 3D Reconstruction using every 5th frame

Prev | Up | Next
TTT.2.2.3 Encoding Details | Home | TTT.2.3 Case #3: Reconstruction From A Sub-region of All Image Frames

DICOM PS3.17 2016e - Explanatory Information