DICOM PS3.4 2016e - Service Class Specifications

S.3.2.4 Get Media Creation Result
Prev | S.3.2 Operations | Next

#### S.3.2.4 Get Media Creation Result

The Get Media Creation Result operation allows an SCU to request of an SCP the status of a media creation request. This operation shall be invoked through the N-GET primitive used in conjunction with the appropriate Media Creation Management SOP Instance corresponding to the creation request.

##### S.3.2.4.1 Attributes

The Application Entity that claims conformance to this SOP Class as an SCU may choose to interpret the Attributes maintained by the SCP that the SCU receives via the operations of the SOP Class. The Application Entity that claims conformance as an SCP to this SOP Class shall support the Attributes specified in Table S.3.2.4.1-1.

Table S.3.2.4.1-1. Media Creation Management SOP Class N-GET Attributes

Attribute Name | Tag | Requirement Type (SCU/SCP)
--- | --- | ---
Specific Character Set | (0008,0005) | 3/1C (Required if expanded or replacement character set is used)
Execution Status | (2100,0020) | 3/1
Execution Status Info | (2100,0030) | 3/1
Total Number of Pieces of Media Created | (2200,000B) | 3/1
Failed SOP Sequence | (0008,1198) | 3/2
Referenced Storage Media Sequence | (2200,000D) | 3/2
All Other Attributes of the Media Creation Management Module |  | 3/3

Prev | Up | Next
S.3.2.3.4 Status Codes | Home | S.3.2.4.2 Service Class User

DICOM PS3.4 2016e - Service Class Specifications