DICOM PS3.3 2016e - Information Object Definitions

C.8.4 Nuclear Medicine Modules
Prev | C.8 Modality Specific Modules | Next

### C.8.4 Nuclear Medicine Modules

This Section describes Nuclear Medicine Series, Equipment, and Image Modules. These Modules contain Attributes that are specific to the NM Image IOD.

### Note

There are some cases where it may be necessary to use several SOP Instances to encode a single NM acquisition. For example, the matrix size must remain constant within a SOP instance. Multiple matrix sizes require multiple SOP instances. Similarly, multiple gated stress levels require separate SOP instances for each stress level. However, a receiving AE is not expected to recombine them.

#### C.8.4.1 NM Series Module (Retired)

This Section was defined in a previous version of the DICOM Standard. The Section is now retired.

Prev | Up | Next
C.8.3 MR Modules | Home | C.8.4.2 NM Equipment Module (Retired)

DICOM PS3.3 2016e - Information Object Definitions