DICOM PS3.17 2016e - Explanatory Information

MM.5 Time Synchronization
Prev | MM Considerations For Applications Creating New Images From Multi-frame Images | Next

## MM.5 Time Synchronization

The time base for the new composite instance should be the same as for the source image and should use the same time synchronization frame of reference. This allows the object to retain synchronization to any simultaneously acquired waveform data

Prev | Up | Next
MM.4 Consistency | Home | MM.6 Audio

DICOM PS3.17 2016e - Explanatory Information