DICOM PS3.4 2016e - Service Class Specifications

EE.3 Conformance
Prev | EE Display System Management Service Class (Normative) | Next

## EE.3 Conformance

### EE.3.1 Conformance Statement

The implementation conformance statement of this SOP class shall follow PS3.2.

The SCU Conformance Statement shall specify the following items:

- Maximum number of associations to be supported at the same time

- List of SOP Classes supported

- For each of the supported SOP classes:

  - List of supported SOP class attributes and DIMSE service elements

  - For each supported attribute (mandatory and optional), a valid value range

The SCP Conformance Statement shall specify the following items:

- Maximum number of associations to be supported at the same time

- List of SOP Classes supported

- For each of the supported SOP classes:

  - List of supported SOP class attributes and DIMSE service elements

  - For each supported attribute (mandatory and optional)

    - Valid value range

    - Default value if no value is supplied by the SCU

    - Status code (Failure or Warning) if the SCU supplies a value that is out of range

- For each supported DIMSE service

  - SCP behavior for all specific status codes

Prev | Up | Next
EE.2.4 Reserved Identifications | Home | FF Volumetric Presentation State Storage SOP Classes (Normative)

DICOM PS3.4 2016e - Service Class Specifications