DICOM PS3.16 2016e - Content Mapping Resource

TID 8140 Heating Conditions
Prev | Acquisition Context SR IOD Templates | Next

### TID 8140 Heating Conditions

This template encodes a description of the heating conditions applied prior to, during or after data acquisition (e.g., during imaging of research small animals).

Type:

  Extensible

Order:

  Non-Significant

Table TID 8140. Heating Conditions

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (127040, DCM, "Heating conditions") | 1 | M |  |
2 | > | CONTAINS | CODE | EV (G-7292, SRT, "Procedure Phase") | 1 | U |  | DCID 631 “Phase of Procedure Requiring Anesthesia”
3 | > | CONTAINS | CODE | EV (C0018851, UMLS, "Heating") | 1 | U |  | DCID 635 “Heating Method”
4 | > | CONTAINS | CODE | EV (127210, DCM, "Feedback temperature regulation") | 1 | U |  | DCID 231 “Yes-No Only”
5 | > | CONTAINS | CODE | EV (C50304, NCIt, "Temperature sensor device component") | 1 | U |  | DCID 636 “Temperature Sensor Device Component Type for Small Animal Procedures”
6 | > | CONTAINS | NUM | EV (F-021FF, SRT, "Equipment Temperature") | 1 | U |  | UNITS = EV (Cel, UCUM, "C")

Content Item Descriptions

Row 2 | Phase during which the conditions are applicable may be implicit in the context of invocation of this template (e.g., TID 8101 “Preclinical Small Animal Image Acquisition Context” Row 7), or explicitly specified.
Row 3 | The definition (from MESH) is "The application of heat to raise the temperature of the environment, ambient or local, or systems for accomplishing this effect".
Row 6 | This is the nominal temperature of the heating device (e.g., heating pad) and/or the set point of the feedback regulation device.

Prev | Up | Next
TID 8131 Medications and Mixture Medications | Home | TID 8150 Circadian Effects

DICOM PS3.16 2016e - Content Mapping Resource