DICOM PS3.3 2016e - Information Object Definitions

C.11.12 Presentation State Shutter Module
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.12 Presentation State Shutter Module

Table C.11.12-1 contains Attributes that specialize Attributes in other Modules included in a Presentation State.

Table C.11.12-1. Presentation State Shutter Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Shutter Presentation Value | (0018,1622) | 1C | A single grayscale unsigned value used to replace those parts of the image occluded by the shutter, when rendered on a monochrome display. The units are specified in P-Values. Required if the Display Shutter Module or Bitmap Display Shutter Module is present. ### Note The requirement in this module is type 1C, which overrides the type 3 in the Display Shutter Module.
Shutter Presentation Color CIELab Value | (0018,1624) | 1C | A color triplet value used to replace those parts of the image occluded by the shutter, when rendered on a color display. The units are specified in PCS-Values, and the value is encoded as CIELab. See Section C.10.7.1.1. Required if the Display Shutter Module or Bitmap Display Shutter Module is present and the SOP Class is other than Grayscale Softcopy Presentation State Storage. ### Note The requirement in this module is type 1C, which overrides the type 3 in the Display Shutter Module and Bitmap Display Shutter Module.

Prev | Up | Next
C.11.11 Presentation State Relationship Module | Home | C.11.13 Presentation State Mask Module

DICOM PS3.3 2016e - Information Object Definitions