DICOM PS3.4 2016e - Service Class Specifications

5.2 Sequences
Prev | 5 Conventions | Next

## 5.2 Sequences

Certain tables in this Part of the DICOM Standard denote a Sequence of Items by using the symbol: '>.'

In Annex A, '>' is used to identify a 'Sequence of Modules.' Nested Sequences of Modules are identified by '>>'. In Annex B and Annex C, '>' is used to identify a 'Sequence of Attributes'. See PS3.5 for the complete specification of how Sequences of Items shall be encoded.

### Note

Information Object Definitions (IODs) that include the Sequence of Module construct are often called folders. The use of 'Sequences of Attributes' is not limited to 'Folders.'

Prev | Up | Next
5 Conventions | Home | 5.3 Response Status Values

DICOM PS3.4 2016e - Service Class Specifications