DICOM PS3.11 2016e - Media Storage Application Profiles

C.4 Spatial Calibration (SC) Class Requirements
Prev | C Ultrasound Application Profile (Normative) | Next

## C.4 Spatial Calibration (SC) Class Requirements

All implementations conforming to the Application Profile Class SC shall include the US Region Calibration Module with the exception of pixel component organization data element (0018,6044) and other data elements that are conditional on that data element.

Prev | Up | Next
C.3.3.2 File Component IDs | Home | C.5 Combined Calibration (CC) Class Requirements

DICOM PS3.11 2016e - Media Storage Application Profiles