DICOM PS3.18 2016e - Web Services

8.2.10 Unique Identifier of the Series Containing the Presentation Object
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.10 Unique Identifier of the Series Containing the Presentation Object

The parameter name shall be "presentationSeriesUID" for URI based mode, and "PresentationSeriesUID" for the WS mode.

Series Instance UID of the series containing the presentation state storage object to be applied on the images. This parameter is REQUIRED and shall only be present if "presentationUID" is present.

If this parameter is present, then the Region of the Image parameter shall not be present. See Section 8.2.4.

The value shall be encoded as a unique identifier (UID) string, as specified in PS3.5, except that it shall not be padded to an even length with a NULL character.

### Note

As specified in DICOM, the Presentation State will be in the same study as the images it applies to.

Prev | Up | Next
8.2.9 Unique Identifier of the Presentation Object | Home | 8.2.11 Transfer Syntax UID

DICOM PS3.18 2016e - Web Services