DICOM PS3.2 2016e - Conformance

I.4.2.2.2 WADO-WS Retrieve Rendered Imaging Document Set
Prev | I.4.2.2 WADO-URI Specification | Next

##### I.4.2.2.2 WADO-WS Retrieve Rendered Imaging Document Set

Table I.4.2-6. WADO-URI Retrieve Rendered Imaging Documents Specification

Parameter | Restrictions
--- | ---
Transfer Syntaxes Supported | Restricted to transfer syntaxes supported by the hosting EXAMPLE-PACS-ARCHIVE
SOP Class restrictions | Restricted to SOP classes supported by the hosting EXAMPLE-PACS-ARCHIVE
Size restriction | Restricted to sizes supported by the hosting EXAMPLE-PACS-ARCHIVE
Rendered formats available | Supports JPEG and PDF for IMAGE IODS, and PDF for non-IMAGE IODS.
Rows restrictions | Must be in range 16 - 32767
Columns restrictions | Must be in range 16 - 32767
Region restrictions | None
Window Center restrictions | Whole window must be in the range of image pixel values.
Window Width restrictions | Must be greater than 4 and whole window must be in the range of image pixel values.
Image Quality restrictions | None
Anonymization | Supports the DICOM Basic Application Level Confidentiality Profile plus the Retain Patient Characteristics option.
Annotation Restrictions | None
Compression available | JPEG
Other restrictions | None

Prev | Up | Next
I.4.2.2 WADO-URI Specification | Home | I.4.2.2.3 WADO-URI Retrieve Imaging Document Set Metadata

DICOM PS3.2 2016e - Conformance