DICOM PS3.4 2016e - Service Class Specifications

CC.2.6.4 Status Codes
Prev | CC.2.6 Set Unified Procedure Step Information (N-SET) | Next

#### CC.2.6.4 Status Codes

The status values that are specific for this DIMSE operation are defined in Table CC.2.6-1. See PS3.7 for additional response status codes.

Table CC.2.6-1. Status Values

Status | Meaning | Code
--- | --- | ---
Success | The requested modification of the Attribute values is performed | 0000
Warning | Requested optional Attributes are not supported. | 0001
Coerced invalid values to valid values | B305
Failure | Refused: The UPS is not in the "IN PROGRESS" state | C310
Refused: The correct Transaction UID was not provided | C301
Refused: The UPS may no longer be updated | C300
Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307

Prev | Up | Next
CC.2.6.3 Service Class Provider Behavior | Home | CC.2.7 Get Unified Procedure Step Information (N-GET)

DICOM PS3.4 2016e - Service Class Specifications