DICOM PS3.8 2016e - Network Communication Support for Message Exchange

5 Conventions
Prev |  | Next

# 5 Conventions

The following conventions are used for the service description tables shown in this part of the Standard.

(=)

  The same parameter value used in the indication or confirmation shall be the same as used in the request or response respectively.

C

  Conditional (on User Option)

M

  Mandatory usage

MF

  Mandatory with a fixed value

NU

  Not Used

P

  Provider Initiated

U

  User Option

UF

  User Option with a fixed value

Blank entries are not applicable.

Prev |  | Next
4 Symbols and Abbreviations | Home | 6 Network Communication Support Environment

DICOM PS3.8 2016e - Network Communication Support for Message Exchange