DICOM PS3.3 2016e - Information Object Definitions

A.32.8 VL Whole Slide Microscopy Image IOD
Prev | A.32 Visible Light Image Information Object Definitions | Next

### A.32.8 VL Whole Slide Microscopy Image IOD

#### A.32.8.1 VL Whole Slide Microscopy Image IOD Description

The VL Whole Slide Microscopy Image IOD specifies the Attributes of a multi-frame visible light whole slide microscopy image encoded as a tiled decomposition. Each frame encodes a single tile within a three-dimensional imaged volume at a uniform resolution.

### Note

An entire set of tiles for an acquisition may be encoded in the frames of a single SOP Instance, in multiple SOP Instances of a single concatenation, or in multiple SOP Instances in a series (with or without concatenations). E.g., a single SOP Instance may contain an entire low resolution image as a single tile (single frame), or a single SOP Instance may contain an entire high resolution, multi-focal depth, multi-spectral acquisition (multiple frames).

Prev | Up | Next
A.32.7.3.2 Image Related Data Encoding | Home | A.32.8.2 VL Whole Slide Microscopy Image IOD Entity-Relationship Model

DICOM PS3.3 2016e - Information Object Definitions