DICOM PS3.4 2016e - Service Class Specifications

CC.2.3.4 Status Codes
Prev | CC.2.3 Subscribe/Unsubscribe to Receive UPS Event Reports (N-ACTION) | Next

#### CC.2.3.4 Status Codes

The status values that are specific for this DIMSE operation are defined in Table CC.2.3-3.

Table CC.2.3-3. Status Values

Status | Meaning | Code
--- | --- | ---
Success | The requested change of subscription state was performed | 0000
Warning | Deletion Lock not granted. | B301
Failure | Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307
Receiving AE-TITLE is Unknown to this SCP | C308
Refused: Specified action not appropriate for specified instance | C314
Refused: SCP does not support Event Reports | C315

Prev | Up | Next
CC.2.3.3 Service Class Provider Behavior | Home | CC.2.4 Report a Change in UPS Status (N-EVENT-REPORT)

DICOM PS3.4 2016e - Service Class Specifications