DICOM PS3.18 2016e - Web Services

8.2.11 Transfer Syntax UID
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.11 Transfer Syntax UID

For the URI service the parameter name shall be "transferSyntax" containing one value.

For the WS service the parameter name shall be "TransferSyntaxUIDList" containing one or more "TransferSyntaxUID" elements.

RS Services shall not support this parameter.

The Transfer Syntax to be used within the DICOM image objects, as specified in PS3.6. This parameter is OPTIONAL for the URI based mode and the WS mode "DICOM Requester" transaction. It shall not be present if contentType is other than application/dicom.

By default the DICOM object(s) returned shall be encoded in Explicit VR Little Endian. Neither Implicit VR, nor Big Endian shall be used. The response shall be the Transfer Syntax requested if possible. If it is not possible for the response to be sent using the requested transfer syntax then the Explicit VR Little Endian Uncompressed Transfer Syntax shall be used.

### Note

The transfer syntax can be one of the JPIP Transfer Syntaxes, in which case the returned objects will contain the URL of the JPIP provider for retrieving the pixel data.

The value(s) shall be encoded as a unique identifier (UID) string, as specified in PS3.5, except that it shall not be padded to an even length with a NULL character.

Prev | Up | Next
8.2.10 Unique Identifier of the Series Containing the Presentation Object | Home | A URI Query Component Syntax (Normative)

DICOM PS3.18 2016e - Web Services