DICOM PS3.3 2016e - Information Object Definitions

C.8.17.4 Ophthalmic Photography Acquisition Parameters Module
Prev | C.8.17 Ophthalmic Photography and Tomography Modules | Next

#### C.8.17.4 Ophthalmic Photography Acquisition Parameters Module

This Module describes patient clinical conditions related to the image acquisition.

Table C.8.17.4-1. Ophthalmic Photography Acquisition Parameters Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Patient Eye Movement Commanded | (0022,0005) | 2 | Enumerated Values: YES NO
Patient Eye Movement Command Code Sequence | (0022,0006) | 1C | Coded value for patient movement or orientation, which is the intent, and not necessarily the result, based on what the patient is capable of. Required if the value of Patient Eye Movement Commanded (0022,0005) is YES. Only a single Item shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID 4201 “Patient Eye Movement Command”.
Include Table C.8.17.8-2 “Ophthalmic Acquisition Parameters Macro Attributes” |

Prev | Up | Next
C.8.17.3 Ophthalmic Photographic Parameters Module | Home | C.8.17.5 Ocular Region Imaged Module

DICOM PS3.3 2016e - Information Object Definitions