DICOM PS3.18 2016e - Web Services

6.5.4 WADO-RS - RetrieveFrames
Prev | 6.5 WADO-RS Request/Response | Next

### 6.5.4 WADO-RS - RetrieveFrames

This action retrieves the DICOM frames for a given study, series, SOP Instance UID, and frame numbers. The response is pixel data, and is encapsulated in a multipart MIME response.

#### 6.5.4.1 Request

The specific Services resources to be used for the RetrieveFrames action shall be as follows:

- Resource

  - {SERVICE}/studies/{StudyInstanceUID}/series/{SeriesInstanceUID}/instances/{SOPInstanceUID}/frames/{FrameList}, where

    - {SERVICE} is the base URL for the service. This may be a combination of protocol (either http or https), host, port, and application.

    - {StudyInstanceUID} is the study instance UID for a single study.

    - {SeriesInstanceUID} is the series instance UID for a single series.

    - {SOPInstanceUID} is the SOP Instance UID for a single SOP Instance.

    - {FrameList} is a comma or %2C separated list of one or more non duplicate frame numbers. These may be in any order (e.g., ../frames/1,2,4,3).

- Method

  - GET

- Headers

  - Accept

    - multipart/related; type="application/octet-stream" [dcm-parameters]

      Specifies that the response can be Little Endian uncompressed pixel data

    - multipart/related; type="{media-type}" [dcm-parameters]

      Specifies that the response can be compressed pixel data encoded using the media types and transfer syntaxes specified in Table 6.1.1.8-3b. See Section 6.1.3.

Prev | Up | Next
6.5.3.2.2 Bulk Data Response | Home | 6.5.4.2 Response

DICOM PS3.18 2016e - Web Services