DICOM PS3.3 2017a - Information Object Definitions

A.42.4 Ophthalmic Photography 16 Bit Image IOD Content Constraints
Prev | A.42 Ophthalmic Photography 16 Bit Image IOD | Next

### A.42.4 Ophthalmic Photography 16 Bit Image IOD Content Constraints

The following constraints on Series and Image attributes take precedence over the descriptions given in the Module Attribute Tables.

#### A.42.4.1 Bits Allocated, Bits Stored, and High Bit

For Ophthalmic Photography 16 bit images, the Enumerated Value of Bits Allocated (0028,0100) (Image Pixel Module, Section C.7.6.3) shall be 16; the Enumerated Value of Bits Stored (0028,0101) shall be 16; and the Enumerated Value of High Bit (0028,0102) shall be 15.

Prev | Up | Next
A.42.3 Ophthalmic Photography 16 Bit Image IOD Modules | Home | A.42.4.2 Contrast/Bolus Agent Sequence

DICOM PS3.3 2017a - Information Object Definitions