DICOM PS3.12 2017a - Media Formats and Physical Media for Media Interchange

F.2.2 Logical Format
Prev | F.2 Media Formats | Next

### F.2.2 Logical Format

The logical format of CD-R shall conform to ISO 9660 level 1, with the extensions described in Section F.2.2.1 through Section F.2.2.2

#### F.2.2.1 System Identifier Field

The ISO 9660 System Identifier Field of the PVD (Primary Volume Descriptor) shall contain "CD-RTOS CD-BRIDGE" if a CD-I (Compact Disc-Interactive) application is present. If a CD-I application is not present, then this field shall be padded with space characters.

Prev | Up | Next
F.2 Media Formats | Home | F.2.2.2 System and Volume Descriptor Area

DICOM PS3.12 2017a - Media Formats and Physical Media for Media Interchange