DICOM PS3.3 2017a - Information Object Definitions

10.24 Device Motion Control Macro
Prev | 10 Miscellaneous Macros | Next

## 10.24 Device Motion Control Macro

Table 10-28 specifies the attributes that describe requirements on performing the movement of a device from an actual to a desired position.

Table 10-28. Device Motion Control Macro Attributes Description

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Device Motion Control Sequence | (300A,0450) | 3 | Device Motion Control Definitions for each degree of freedom. One or more Items are permitted in this Sequence.
>Device Motion Parameter Code Sequence | (300A,0453) | 1 | The parameter for which the Device Motion Control shall be applied.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Defined CID 9401 “IEC61217 Device Position Parameters”
>Device Motion Execution Mode | (300A,0451) | 1C | Permitted Motion Execution Mode for movement. Required if Device Motion Observation Mode (300A,0452) is absent. May be present otherwise. See Section 10.24.1.1.
>Device Motion Observation Mode | (300A,0452) | 1C | Required Motion Observation Mode for movement. Required if Device Motion Execution Mode (300A,0451) is absent. May be present otherwise. See Section 10.24.1.2.

### 10.24.1 Device Motion Control Macro Attributes

#### 10.24.1.1 Device Motion Execution Mode

Device Motion Execution Mode (300A,0451) identifies how the operator invokes and controls the motion.

Enumerated Values:

CONTINUOUS

  The device must be moved while the operator is activating one or more switches on the machine during the whole period of movement to prevent any uncontrolled movement.

TRIGGERED

  The device can be moved automatically to the desired position, triggered by a one-time command of the operator, without the need to constantly activate any switch.

AUTOMATIC

  The device movement can be initiated and performed automatically by the device to the desired position.

#### 10.24.1.2 Device Motion Observation Mode

Device Motion Observation Mode (300A,0452) describes the presence of the operator in the room, observing the motion.

Enumerated Values:

INROOM

  The movement of the device is only allowed when the operator is present in the treatment room.

REMOTE

  The device can be moved by a command of the operator not being present in the treatment room, that is, from a device outside the treatment room.

Prev | Up | Next
10.23 RT Equipment Correlation Macro | Home | 10.25 Attribute Value Constraint Macro

DICOM PS3.3 2017a - Information Object Definitions