DICOM PS3.17 2017a - Explanatory Information

XXX.5.3 Pass-through Compositing
Prev | XXX.5 Compositing and the Use of Weighting Transfer Functions | Next

### XXX.5.3 Pass-through Compositing

In this example, each channel's Alpha value becomes the weighting factor for that channel.

Figure XXX.5-3. Weighting LUTs for Pass-Through Compositing

Prev | Up | Next
XXX.5.2 Partially Transparent A Over B Compositing | Home | XXX.5.4 Threshold Compositing

DICOM PS3.17 2017a - Explanatory Information