DICOM PS3.16 2017a - Content Mapping Resource

CID 3672 Pacemakers
Prev | B DCMR Context Groups (Normative) | Next

## CID 3672 Pacemakers

This Context Group includes the full set of codes for types of pacemakers specified in the NASPE/BPEG Generic Pacemaker Code (NBG). The Coding Scheme Designator (0008,0102) shall be NBG.

### Note

1. A prior version of this context group used codes from the SCP-ECG vocabulary.

2. Further information at http://www.hrsonline.org/Practice-Guidance/Clinical-Guidelines-Documents/2002-The-Revised-NASPE-BPEG-Generic-Code-for-Antibradycardia-AdaptiveRate-and-Multisite-Pacing. For reference, the scheme is reproduced here:

   Code Position | 1 - Chamber(s) paced | 2 - Chamber(s) sensed | 3 - Response to sensing | 4 - Rate modulation | 5- Multisite pacing
   Code values | O = None A = Atrium V = Ventricle D = Dual (A+V) S = Single(A or V - Mfr designation only) | O = None A = Atrium V = Ventricle D = Dual (A+V) S = Single(A or V - Mfr designation only) | O = None T = Triggered I = Inhibited D = Dual (T+I) | O = None R = Rate modulation | O = None A = Atrium V = Ventricle D = Dual (A+V)

Prev | Up | Next
CID 3671 Reason for ECG Exam | Home | CID 3673 Diagnosis (Retired)

DICOM PS3.16 2017a - Content Mapping Resource