DICOM PS3.3 2017a - Information Object Definitions

A.34.2.4.4 Sampling Frequency
Prev | A.34.2.4 Basic Voice Audio IOD Content Constraints | Next

##### A.34.2.4.4 Sampling Frequency

The value of Sampling Frequency (003A,001A) in the Waveform Sequence Item shall be 8000.

Prev | Up | Next
A.34.2.4.3 Number of Waveform Channels | Home | A.34.2.4.5 Waveform Sample Interpretation

DICOM PS3.3 2017a - Information Object Definitions