DICOM PS3.2 2017a - Conformance

G.4.4.2 Parameters
Prev | G.4.4 Configuration | Next

#### G.4.4.2 Parameters

Table G.4.4-1. Configuration Parameters Table

Parameter | Configurable | Default Value
--- | --- | ---
General Parameters
PDU Size | No | 16kB
Time-out waiting for acceptance or rejection Response to an Association Open Request. (Application Level timeout) | No | None
General DIMSE level time-out values | No | None
Time-out waiting for response to TCP/IP connect() request. (Low-level timeout) | No | None
Time-out waiting for acceptance of a TCP/IP message over the network. (Low-level timeout) | No | None
Time-out for waiting for data between TCP/IP packets. (Low-level timeout) | No | None
Any changes to default TCP/IP settings, such as configurable stack parameters. | No | None
AE Specific Parameters (all AEs)
Size constraint in maximum object size | No | None
Maximum PDU size the AE can receive (see note 1) | No | Unlimited
Maximum PDU size the AE can send | No | Unlimited
AE specific DIMSE level time-out values | No | None
Number of simultaneous Associations by Service and/or SOP Class | No | Unlimited
SOP Class support | No | All supported SOP Classes always proposed and accepted
Transfer Syntax support | No | All supported Transfer Syntaxes always proposed and accepted
Other parameters that are configurable | No | None

### Note

Though the application can support unlimited PDU sizes, it will never offer a Maximum Received PDU Length of zero (unlimited) since this triggers a bug in some older systems.

Prev | Up | Next
G.4.4 Configuration | Home | G.5 Media Interchange

DICOM PS3.2 2017a - Conformance