DICOM PS3.3 2017a - Information Object Definitions

C.8.8.29.2 Adjusted Table Positions and Angles
Prev | C.8.8.29 RT Beams Delivery Instruction Module | Next

##### C.8.8.29.2 Adjusted Table Positions and Angles

Adjusted Table positions and angles serve as a facility to communicate a shift (often systematic) that has been detected from previous treatments. They define a new initial patient position, which is near and aligned to the actual patient position during beam delivery. These attributes do not affect the original relationship between the beams and the planning image patient anatomy.

Prev | Up | Next
C.8.8.29 RT Beams Delivery Instruction Module | Home | C.8.8.29.3 Meterset Exposure

DICOM PS3.3 2017a - Information Object Definitions