DICOM PS3.3 2017a - Information Object Definitions

A.34.10.4.4 Sampling Frequency
Prev | A.34.10.4 General Audio Waveform IOD Content Constraints | Next

##### A.34.10.4.4 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item shall be less than or equal to 44,100 Hz.

Prev | Up | Next
A.34.10.4.3 Number of Waveform Channels | Home | A.34.10.4.5 Channel Source

DICOM PS3.3 2017a - Information Object Definitions