DICOM PS3.16 2017b - Content Mapping Resource

CID 6 Transducer Orientation
Prev | B DCMR Context Groups (Normative) | Next

## CID 6 Transducer Orientation

Type:

  Extensible

Version:

  20040322

Table CID 6. Transducer Orientation

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-CT Concept ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
SRT | G-A138 | Coronal | 81654009 | C0205123
SRT | G-A143 | Longitudinal | 38717003 | C0205127
SRT | G-A145 | Sagittal | 30730003 | C0205129
SRT | G-A189 | Parasagittal | 103343002 | C0522491
SRT | G-A472 | Oblique | 21114003 | C0205315
SRT | G-A185 | Long axis | 103339001 | C0522487
SRT | G-A13B | Off axis | 419161000 | C1635161
SRT | G-A186 | Short axis | 103340004 | C0522488
SRT | G-A191 | Five chamber | 398994001 | C1302157
SRT | G-A19B | Two chamber | 399232001 | C1302267
SRT | G-A19C | Four chamber | 399214001 | C1302256
SRT | G-A117 | Transverse | 62824007 | C0205106

### Note

In a prior version of this table, the code G-A11B was specified for the concept Parasagittal. The use of this code conflicts with its assignment to another concept in SNOMED, and its use in this context is deprecated. Although there is minimal possibility of misinterpretation with SOP Instances that may include the deprecated use, receiving applications should be aware of this change; see Annex J.

Prev | Up | Next
CID 5 Transducer Approach | Home | CID 7 Ultrasound Beam Path

DICOM PS3.16 2017b - Content Mapping Resource