DICOM PS3.17 2017b - Explanatory Information

TTT.2.7.3 Encoding Details
Prev | TTT.2.7 Case #7: Spatial Registration of 3D X-Ray Angiography With Enhanced XA | Next

#### TTT.2.7.3 Encoding Details

##### TTT.2.7.3.1 Enhanced X-Ray Angiographic Image IOD

This scenario is based on the encoding of the 2D acquisition as an Enhanced XA Image, containing the attributes of the X-Ray Isocenter Reference System Macro (see Section C.8.19.6.13 “X-Ray Isocenter Reference System Macro” in PS3.3 ).

Prev | Up | Next
TTT.2.7.2 Encoding Outline | Home | TTT.2.7.3.2 X-Ray 3D Angiographic Image IOD

DICOM PS3.17 2017b - Explanatory Information