DICOM PS3.15 2017b - Security and System Management Profiles

B.6 Kerberos Identity Negotiation Association Profile
Prev | B Secure Transport Connection Profiles (Normative) | Next

## B.6 Kerberos Identity Negotiation Association Profile

An implementation that supports the Kerberos Identity Negotiation Association Profile shall send/accept the User Identity association negotiation sub-item, for User-Identity-Type of 3. If a positive response is requested, the association acceptor implementation shall respond with the association response sub-item containing a Kerberos server ticket. The Kerberos server ticket information shall be made available to internal or external Kerberos authentication systems. The user identity shall be authenticated by means of the Kerberos authentication system. If the authentication fails, the association shall be rejected.

The user identity from the Primary-field shall be used within the implementation as the user identification. Such uses include recording user identification in audit messages.

Table B.6-1. Kerberos Identity Negotiation Association Profile - Minimum Mechanisms for DICOM Association Negotiation Features

Supported Association Negotiation Feature | Minimum Mechanism
--- | ---
User Identity | Kerberos

Prev | Up | Next
B.5 User Identity Plus Passcode Association Profile | Home | B.7 Generic SAML Assertion Identity Negotiation Association Profile

DICOM PS3.15 2017b - Security and System Management Profiles