DICOM PS3.3 2017b - Information Object Definitions

A.52.3 Ophthalmic Tomography Image IOD Modules
Prev | A.52 Ophthalmic Tomography Image IOD | Next

### A.52.3 Ophthalmic Tomography Image IOD Modules

Table A.52.3-1. Ophthalmic Tomography Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Ophthalmic Tomography Series | C.8.17.6 | M
Frame of Reference | Frame of Reference | C.7.4.1 | C - Required if Ophthalmic Photography Reference Image available or if Ophthalmic Volumetric Properties Flag (0022,1622) is YES. May be present otherwise.
Synchronization | C.7.4.2 | C - Required if Ophthalmic Photography Reference Image available
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Image Pixel | C.7.6.3 | M
Enhanced Contrast/Bolus | C.7.6.4b | C - Required if contrast was administered
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | M
Acquisition Context | C.7.6.14 | M
Cardiac Synchronization | C.7.6.18.1 | C - Required if cardiac synchronization was used
Ophthalmic Tomography Image | C.8.17.7 | M
Ophthalmic Tomography Acquisition Parameters | C.8.17.8 | M
Ophthalmic Tomography Parameters | C.8.17.9 | M
Ocular Region Imaged | C.8.17.5 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

Prev | Up | Next
A.52.2 Ophthalmic Tomography Image IOD Entity-Relationship Model | Home | A.52.4 Ophthalmic Tomography Image IOD Content Constraints

DICOM PS3.3 2017b - Information Object Definitions