DICOM PS3.11 2017b - Media Storage Application Profiles

C.3.3.2 File Component IDs
Prev | C.3.3 DICOMDIR | Next

#### C.3.3.2 File Component IDs

### Note

File Component IDs should be created using a random number filename to minimize File Component ID collisions as described in PS3.12. The FS-Updater should check the existence of a Component ID prior to creating that ID. Should an ID collision occur, the FS-Updater should try another ID.

Prev | Up | Next
C.3.3 DICOMDIR | Home | C.4 Spatial Calibration (SC) Class Requirements

DICOM PS3.11 2017b - Media Storage Application Profiles