DICOM PS3.3 2017b - Information Object Definitions

A.34.5.4.5 Sampling Frequency
Prev | A.34.5.4 Ambulatory ECG IOD Content Constraints | Next

##### A.34.5.4.5 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item shall be between 50 and 1000, inclusive.

Prev | Up | Next
A.34.5.4.3 Number of Waveform Channels | Home | A.34.5.4.6 Channel Source

DICOM PS3.3 2017b - Information Object Definitions