DICOM PS3.4 2017b - Service Class Specifications

CC.2.7.4 Status Codes
Prev | CC.2.7 Get Unified Procedure Step Information (N-GET) | Next

#### CC.2.7.4 Status Codes

The status values that are specific for this DIMSE operation are defined in Table CC.2.7-1. See PS3.7 for additional response status codes.

Table CC.2.7-1. Status Values

Status | Meaning | Code
--- | --- | ---
Warning | Requested optional Attributes are not supported | 0001
Failure | Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307

Prev | Up | Next
CC.2.7.3 Service Class Provider Behavior | Home | CC.2.8 Search for Unified Procedure Step (C-FIND)

DICOM PS3.4 2017b - Service Class Specifications