DICOM PS3.3 2017b - Information Object Definitions

A.67.3 Ophthalmic Thickness Map IOD Modules
Prev | A.67 Ophthalmic Thickness Map IOD | Next

### A.67.3 Ophthalmic Thickness Map IOD Modules

Table A.67.3-1 specifies the Modules of the Ophthalmic Thickness Map IOD.

Table A.67.3-1. Ophthalmic Thickness Map IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Ophthalmic Thickness Map Series | C.8.28.1 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Supplemental Palette Color Lookup Table | C.7.6.19 | C - Required if Pixel Presentation (0008,9205) equals COLOR
Bitmap Display Shutter | C.7.6.15 | C - Required if a Shutter is to be applied to the image
Ophthalmic Thickness Map | C.8.28.2 | M
Ophthalmic Thickness Map Quality Rating | C.8.28.3 | C - Required if a quality rating value exists for the ophthalmic map
Ophthalmic Photography Acquisition Parameters | C.8.17.4 | M
Acquisition Context | C.7.6.14 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

Prev | Up | Next
A.67.2 Ophthalmic Thickness Map IOD Entity-Relationship Model | Home | A.67.4 Ophthalmic Thickness Map IOD Content Constraints

DICOM PS3.3 2017b - Information Object Definitions