DICOM PS3.18 2017e - Web Services

6.5.2.2.2 Bulk Data Response
Prev | 6.5.2.2 Response | Next

##### 6.5.2.2.2 Bulk Data Response

- Content-Type:

  - multipart/related; type="application/octet-stream"; boundary={MessageBoundary}

  - multipart/related; type="{media-type}"; boundary={MessageBoundary} [dcm-parameters]

  See Section 6.1.3.

- The entire multipart response contains all bulk data for the specified Series that can be converted to one of the requested media types.

- Each item in the response is one of:

  - an uncompressed bulk data element encoded in Little Endian binary format with the following headers:

    - Content-Type: application/octet-stream

    - Content-Location: {BulkDataURI}

  - an Encapsulated Document (0042,0011) bulk data element from a SOP Instance in the Series encoded in the media type specified in MIME Type of Encapsulated Document (0042,0012) in the Instance with the following header fields:

    - Content-Type: {media-type}

    - Content-Location: {BulkDataURI}

  - a compressed bulk data element from a SOP Instance in the Series encoded in a single-frame media type with the following headers:

    - Content-Type: {media-type} [dcm-parameters]

    - Content-Location: {BulkDataURI}

  - a compressed frame from a multi-frame SOP Instance in the Series encoded in a single-frame media type with the following headers:

    - Content-Type: {media-type} [dcm-parameters]

    - Content-Location: {BulkDataURI}/frames/{FrameNumber}

  - all of the compressed frames from a multi-frame SOP Instance in the Series encoded in a video media type with the following headers:

    - Content-Type: {media-type} [dcm-parameters]

    - Content-Location: {BulkDataURI}

Prev | Up | Next
6.5.2.2 Response | Home | 6.5.3 WADO-RS - RetrieveInstance

DICOM PS3.18 2017e - Web Services