DICOM PS3.18 2017e - Web Services

8.2.7 Frame Number
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.7 Frame Number

The parameter name shall be "frameNumber" for URI mode.

Specifies that the single frame with that number within a multi-frame image object, as defined in PS3.3 that shall be returned. It is OPTIONAL. It shall not be present if contentType is application/dicom.

If the target resource is:

- a single frame image and the frame number is present and not 1, or

- a multi-frame image and the frame number is not between 1 and the number of frames in the image (inclusive), or

- not an image

then the response shall be a 400 (Bad Request), and may include a payload containing an appropriate error message.

The value shall be encoded as an integer string (IS), as specified in PS3.5.

Prev | Up | Next
8.2.6 Reserved | Home | 8.2.8 Image Quality

DICOM PS3.18 2017e - Web Services