DICOM PS3.17 2017e - Explanatory Information

XXX.3.9.3.2 Volumetric Presentation State Relationship Module Recommendations
Prev | XXX.3.9.3 Encoding Details | Next

##### XXX.3.9.3.2 Volumetric Presentation State Relationship Module Recommendations

Table XXX.3.9-2. Volumetric Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Volumetric Presentation State Input Sequence | (0070,1201) | Each VPS contains a single Input Sequence item referencing a single phase within a multiphase acquisition.
>Referenced Image Sequence | (0008,1140) | Set reference(s) to the image(s) that make up the input volume for this phase.

Prev | Up | Next
XXX.3.9.3 Encoding Details | Home | XXX.3.9.3.3 Presentation View Description Module Recommendations

DICOM PS3.17 2017e - Explanatory Information