DICOM PS3.3 2017e - Information Object Definitions

C.8.27.2.3 Pixel Presentation
Prev | C.8.27.2 Intravascular OCT Image Module | Next

##### C.8.27.2.3 Pixel Presentation

Pixel Presentation (0008,9205) is used to indicate whether a color tint is intended to be applied to the IVOCT image. See Table C.8.27.2-4.

Table C.8.27.2-4. Pixel Presentation Attribute Values

Enumerated Value Name | Enumerated Value Description
--- | ---
COLOR | Image is intended to be displayed in color using Supplemental Palette Color LUTs, but can be displayed in grayscale if current display does not support color or with a user selected LUT. See Section C.8.16.2.1.1.1.
COLOR_REF | Image is intended to be displayed in color using an externally defined Palette Color LUTs, but can be displayed in grayscale if current display does not support color, or with a user selected LUT. I.e., the encoded pixel values are still continuous grayscale values (and not arbitrarily order indices into a lookup table).
MONOCHROME | Image is intended to be displayed in grayscale only.

Prev | Up | Next
C.8.27.2.2 Volumetric Properties | Home | C.8.27.2.4 Bits Allocated, Bits Stored and Samples Per Pixel

DICOM PS3.3 2017e - Information Object Definitions